| CAEN FERS Library v1.1.4 SDK for FERS systems

Functions
Read sensors temperature
API
Collaboration diagram for Read sensors temperature:

## Functions
int | FERS_Get_TDC0_Temp (int handle, float *temp)
| Get the temperature from picoTDC0 (on the board) More...
int | FERS_Get_TDC1_Temp (int handle, float *temp)
| Get the temperature from picoTDC1 (on the mezzanine) More...
int | FERS_Get_FPGA_Temp (int handle, float *temp)
| Get FPGA die temperature. More...
int | FERS_Get_Board_Temp (int handle, float *temp)
| Get Board temperature, between PIC and FPGA. More...

## Detailed Description

## Function Documentation

## ◆ FERS_Get_TDC0_Temp()

int FERS_Get_TDC0_Temp | ( | int | handle,
|  | float * | temp
| ) |  |

Get the temperature from picoTDC0 (on the board)

Parameters

  [out] | temp | TDC temperature in Celsiuse
  [in] | handle | Handle to the FERS device

Returns
  0 on success, or a negative error code as defined in FERSLIB_ErrorCodes

## ◆ FERS_Get_TDC1_Temp()

int FERS_Get_TDC1_Temp | ( | int | handle,
|  | float * | temp
| ) |  |

Get the temperature from picoTDC1 (on the mezzanine)

Parameters

  [out] | temp | TDC temperature in Celsius
  [in] | handle | Handle to the FERS device

Returns
  0 on success, or a negative error code as defined in FERSLIB_ErrorCodes

## ◆ FERS_Get_FPGA_Temp()

int FERS_Get_FPGA_Temp | ( | int | handle,
|  | float * | temp
| ) |  |

Get FPGA die temperature.

Parameters

  [out] | temp | FPGA temperature in Celsius
  [in] | handle | device handle

Returns
  0

## ◆ FERS_Get_Board_Temp()

int FERS_Get_Board_Temp | ( | int | handle,
|  | float * | temp
| ) |  |

Get Board temperature, between PIC and FPGA.

Parameters

  [out] | temp | PIC board temperature in Celsius
  [in] | handle | device handle

Returns
  0