| CAEN FERS Library v1.1.4 SDK for FERS systems

Macros
Measurement modes
Macros

Measurement modes for 5203. More...

Collaboration diagram for Measurement modes:

## Macros
#define | MEASMODE_LEAD_ONLY 0x01
#define | MEASMODE_LEAD_TRAIL 0x03
#define | MEASMODE_LEAD_TOT8 0x05
#define | MEASMODE_LEAD_TOT11 0x09
#define | MEASMODE_OWLT(m) (((m) == MEASMODE_LEAD_TOT8) || ((m) == MEASMODE_LEAD_TOT11)) /*! True if TDC MeasMode includes ToT */

## Detailed Description

Measurement modes for 5203.

## Macro Definition Documentation

## ◆ MEASMODE_LEAD_ONLY

#define MEASMODE_LEAD_ONLY 0x01

Leading edge only mode

Definition at line 321 of file FERSlib.h.

## ◆ MEASMODE_LEAD_TRAIL

#define MEASMODE_LEAD_TRAIL 0x03

Leading and trailing edges mode

Definition at line 322 of file FERSlib.h.

## ◆ MEASMODE_LEAD_TOT8

#define MEASMODE_LEAD_TOT8 0x05

Leading edge + ToT 8 bits mode

Definition at line 323 of file FERSlib.h.

## ◆ MEASMODE_LEAD_TOT11

#define MEASMODE_LEAD_TOT11 0x09

Leading edge + ToT 11 bits mode

Definition at line 324 of file FERSlib.h.

## ◆ MEASMODE_OWLT

#define MEASMODE_OWLT | ( |  | m | ) | (((m) == MEASMODE_LEAD_TOT8) || ((m) == MEASMODE_LEAD_TOT11)) /*! True if TDC MeasMode includes ToT */

Definition at line 325 of file FERSlib.h.