| CAEN FERS Library v1.1.4 SDK for FERS systems

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - t -

- T0_outMask : Config_t
- T1_outMask : Config_t
- T_Gain : Config_t
- t_or_cnt : ServEvent_t
- t_or_counts : CountingEvent_t
- TD1_CoarseThreshold : Config_t
- TD1_FineThreshold : Config_t
- TD1_Mask : Config_t
- TD2_CoarseThreshold : Config_t
- TD2_FineThreshold : Config_t
- TD2_Mask : Config_t
- TD_CoarseThreshold : Config_t
- TD_FineThreshold : Config_t
- TD_Mask : Config_t
- TDC_ChBufferSize : Config_t
- TDCpulser_Period : Config_t
- TDCpulser_Width : Config_t
- TDCROStatus : ServEvent_t
- TdlClkPhase : Config_t
- tempBoard : ServEvent_t
- tempDetector : ServEvent_t
- TempFeedbackCoeff : Config_t
- tempFPGA : ServEvent_t
- tempHV : ServEvent_t
- TempSensCoeff : Config_t
- tempTDC : ServEvent_t
- test_data : TestEvent_t
- TestMode : Config_t
- TestPulseAmplitude : Config_t
- TestPulseDestination : Config_t
- TestPulsePreamp : Config_t
- TestPulseSource : Config_t
- tg_bot_nen_coarse : picoTDC_Cfg_t
- tg_bot_nen_fine : picoTDC_Cfg_t
- tg_cal_nrst : picoTDC_Cfg_t
- tg_cal_parity_in : picoTDC_Cfg_t
- tg_delay_taps : picoTDC_Cfg_t
- tg_top_nen_coarse : picoTDC_Cfg_t
- tg_top_nen_fine : picoTDC_Cfg_t
- Tlogic_Mask : Config_t
- Tlogic_Width : Config_t
- ToA : ListEvent_t
- ToT : ListEvent_t
- tot : picoTDC_Cfg_t
- ToT : SpectEvent_t
- tot_8bit : picoTDC_Cfg_t
- tot_leadingstartbit : picoTDC_Cfg_t
- ToT_LSB : Config_t
- ToT_reject_high_thr : Config_t
- ToT_reject_low_thr : Config_t
- tot_saturate : picoTDC_Cfg_t
- tot_startbit : picoTDC_Cfg_t
- TOTD_CoarseThreshold : Config_t
- TOTD_FineThreshold : Config_t
- TOTD_Mask : Config_t
- TotTrg_cnt : ServEvent_t
- tr_dropped : picoTDC_Cfg_t
- tr_fillgrade : picoTDC_Cfg_t
- tr_parity : picoTDC_Cfg_t
- tr_stateerr : picoTDC_Cfg_t
- trailer : ListEvent_t
- Tref_Mask : Config_t
- Tref_tstamp : ListEvent_t
- TrefDelay : Config_t
- TrefWindow : Config_t
- Trg0Del_ToT : picoTDC_Cfg_t
- trg_ch0_delay : picoTDC_Cfg_t
- Trg_Status : picoTDC_Cfg_t
- TrgHoldOff : Config_t
- TrgIdMode : Config_t
- TrgWindow : picoTDC_Cfg_t
- TrgWindowOffset : Config_t
- TrgWindowWidth : Config_t
- trig_phase : picoTDC_Cfg_t
- trigger_buffer_size : picoTDC_Cfg_t
- trigger_ch0_en : picoTDC_Cfg_t
- trigger_create : picoTDC_Cfg_t
- trigger_create_single : picoTDC_Cfg_t
- trigger_id : CountingEvent_t, ListEvent_t, SpectEvent_t, TestEvent_t, WaveEvent_t
- trigger_latency : picoTDC_Cfg_t
- trigger_window : picoTDC_Cfg_t
- TriggerBufferSize : Config_t
- TriggerLogic : Config_t
- TriggerMask : Config_t
- tstamp : ListEvent_t, SpectEvent_t
- tstamp_clk : ListEvent_t
- tstamp_us : CountingEvent_t, ListEvent_t, ServEvent_t, SpectEvent_t, TestEvent_t, WaveEvent_t
- tx_strenght : picoTDC_Cfg_t