| CAEN FERS Library v1.1.4 SDK for FERS systems

Macros
FERS_Registers_5215.h File Reference
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | _REGISTERS_5215_H
#define | VR_IO_STANDARD 0
#define | VR_IO_FA_DIR 1
#define | VR_IO_FB_DIR 2
#define | VR_IO_RA_DIR 3
#define | VR_IO_RB_DIR 4
#define | VR_IO_FA_FN 5
#define | VR_IO_FB_FN 6
#define | VR_IO_RA_FN 7
#define | VR_IO_RB_FN 8
#define | VR_IO_FOUT_FN 9
#define | VR_IO_VETO_FN 10
#define | VR_IO_FIN_MASK 11
#define | VR_IO_FOUT_MASK 12
#define | VR_IO_REG_VALUE 13
#define | VR_IO_TP_PERIOD 14
#define | VR_IO_TP_WIDTH 15
#define | VR_IO_CLK_SOURCE 16
#define | VR_IO_SYNC_OUT_A_FN 17
#define | VR_IO_SYNC_OUT_B_FN 18
#define | VR_IO_SYNC_OUT_C_FN 19
#define | VR_IO_MASTER_SALVE 20
#define | VR_IO_SYNC_PULSE_WIDTH 21
#define | VR_IO_SYNC_SEND 22
#define | VR_SYNC_DELAY 23
#define | VR_FIN_MAJORITY 24
#define | VR_IO_PPS_SOURCE 25
#define | VR_IO_PLL_STATUS 26
#define | VR_IO_LED_TEST_1 27
#define | VR_IO_LED_TEST_2 28
#define | VR_DMA_FLAGS_INFO 29
#define | VR_DMA_FLAGS_DATA 30
#define | VR_ENABLED_LINKS 31
#define | VR_IO_DEBUG 32
#define | VR_IO_SYNCSOURCE_ZERO 0
#define | VR_IO_SYNCSOURCE_SW_PULSE 1
#define | VR_IO_SYNCSOURCE_SW_REG 2
#define | VR_IO_SYNCSOURCE_FA 3
#define | VR_IO_SYNCSOURCE_FB 4
#define | VR_IO_SYNCSOURCE_RA 5
#define | VR_IO_SYNCSOURCE_RB 6
#define | VR_IO_SYNCSOURCE_GPS_PPS 7
#define | VR_IO_SYNCSOURCE_CLK_REF 8
#define | VR_IO_BOARD_MODE_MASTER 0
#define | VR_IO_BOARD_MODE_SLAVE 1
#define | VR_IO_STANDARD_IO_NIM 0
#define | VR_IO_STANDARD_IO_TLL 1
#define | VR_IO_DIRECTION_OUT 0
#define | VR_IO_DIRECTION_IN_R50 1
#define | VR_IO_DIRECTION_IN_HIZ 2
#define | VR_IO_FUNCTION_REGISTER 0
#define | VR_IO_FUNCTION_LOGIC_OR 1
#define | VR_IO_FUNCTION_LOGIC_AND 2
#define | VR_IO_FUNCTION_MAJORITY 3
#define | VR_IO_FUNCTION_TEST_PULSE 4
#define | VR_IO_FUNCTION_SYNC 5
#define | VR_IO_FUNCTION_FA_IN 6
#define | VR_IO_FUNCTION_FB_IN 7
#define | VR_IO_FUNCTION_RA_IN 8
#define | VR_IO_FUNCTION_RB_IN 9
#define | VR_IO_FUNCTION_ZERO 15
#define | VR_IO_CLKSOURCE_INTERNAL 0
#define | VR_IO_CLKSOURCE_LEMO 1
#define | VR_IO_CLKSOURCE_SYNC 2
#define | VR_IO_CLKSOURCE_RA 3
#define | VR_DPROBE_MON_TX_SYNC_SHORT 0x01
| sending periodic synch (short) More...
#define | VR_DPROBE_MON_TX_SYNC_ALIGN 0x02
| link alignment in progress More...
#define | VR_DPROBE_MON_TX_SYNC_LONG 0x03
| sending periodic synch (long) More...
#define | VR_DPROBE_MON_TX_TIMING_SEND 0x04
| sending Timing *T0 More...
#define | VR_DPROBE_MON_TX_NORMAL_SEND 0x05
| FSM low level TX is in the state ready to transmit standard packets (reg/cmd) More...
#define | VR_DPROBE_MON_TX_TLAST_SEND 0x06
| FSM low level TX is transmetting last word. More...
#define | VR_DPROBE_MON_TX_DATA_SEND 0x07
| FSM low level TX is transmetting a standard packets (reg/cmd) More...
#define | VR_DPROBE_MON_TX_SYNC_PENDING 0x08
| Periodic synch is pending. More...
#define | VR_DPROBE_MON_TX_FIFOFULL 0x09
| TX fifo full, commands and re access will be lost. More...
#define | VR_DPROBE_MON_TX_TVALID 0x0A
| tvalid fifo tx More...
#define | VR_DPROBE_MON_TX_TREADY 0x0B
| tready fifo tx More...
#define | VR_DPROBE_SC_BUSY 0x10
| register cmd interface busy More...
#define | VR_DPROBE_SC_DATA_WR 0x11
| data to write More...
#define | VR_DPROBE_SC_INT_RD 0x12
| read operation request More...
#define | VR_DPROBE_SC_INT_WR 0x13
| write operation request More...
#define | VR_DPROBE_SC_COMMIT 0x14
| packet commit More...
#define | VR_DPROBE_SC_ACK 0x15
| ack to commit request More...
#define | VR_DPROBE_SC_NACK 0x16
| nack to commit request More...
#define | VR_DPROBE_STR_SOP 0x17
| start incoming data packet More...
#define | VR_DPROBE_STR_EOP 0x18
| end incoming data packet More...
#define | VR_DPROBE_STR_EOB 0x19
| end of train More...
#define | VR_DPROBE_STR_DATA_VALID 0x20
| data valid (read) More...
#define | VR_DPROBE_CMD_BUSY 0x21
| command interface busy More...
#define | VR_DPROBE_CMD_COMMIT 0x22
| sending command from CPU More...
#define | VR_DPROBE_ENUMERATEBOARD 0x23
| request of enumeration More...
#define | VR_DPROBE_ENUMERATION_COMPLETED 0x24
| enumeration completed More...
#define | VR_DPROBE_SEND_T0 0x25
| send T0 More...
#define | VR_DPROBE_G_REINIT_LINK 0x26
| reinitialize link More...
#define | VR_DPROBE_READOUT_READY 0x27
| readout ready More...
#define | VR_DPROBE_MON_AXSM_WRITEREG 0x30
| FSM protocol is sending a reg read. More...
#define | VR_DPROBE_MON_AXSM_READREG 0x31
| FSM protocol is sending a reg write. More...
#define | VR_DPROBE_MON_AXSM_SENDCMD 0x32
| FSM protocol is sending a command. More...
#define | VR_DPROBE_MON_AXSM_SENDTOKEN 0x33
| FSM protocol is sending a token (start of train) More...
#define | VR_DPROBE_MON_AXSM_PENDING_TOKEN 0x34
| a token is pending (= is circulating) More...
#define | VR_DPROBE_MON_AXSM_PENDING_REG 0x35
| pending send register More...
#define | CNC_STATUS_INVALID_CHAIN 1
#define | CNC_STATUS_INVALID_BOARD 2
#define | CNC_STATUS_INVALID_FIRMWARE 3
#define | CNC_STATUS_CHAIN_NOT_INITIALIZED 4
#define | CNC_STATUS_UNABLE_TO_MAP_MEMORY_TO_USER_SPACE 5
#define | CNC_STATUS_UNABLE_TO_OPEN_DEV_MEM 6
#define | CNC_STATUS_UNABLE_TO_ALLOCATE_USER_MEMORY 7
#define | CNC_STATUS_UANBLE_TO_ALLOCATE_KERNEL_MEMORY 8
#define | CNC_STATUS_MEMORY_NOT_MAPPED 9
#define | CNC_STATUS_ADDRESS_OUT_OF_MEMORY 10
#define | CNC_STATUS_NO_MORE_SPACE 11
#define | CNC_STATUS_EMPTY 12
#define | CNC_STATUS_FULL 13
#define | CNC_STATUS_INVALID_SETTINGS 14
#define | CNC_STATUS_NO_MORE_SPACE_IN_THE_LIST 15
#define | CNC_STATUS_LIST_ALMOST_FULL 16
#define | CNC_STATUS_DMA_FAILED 17
#define | CNC_STATUS_CHAIN_DOWN 18
#define | CNC_STATUS_INVALID_IO_MODE 19
#define | CNC_STATUS_FPGA_IO_ERROR 20
#define | CNC_STATUS_IIC_IO_ERROR 21
#define | CNC_STATUS_INVALID_REGISTER 22
#define | CNC_STATUS_LINK_ERROR 23
#define | CNC_STATUS_UNABLE_TO_SET_LINK_PROP_DELAY 24
#define | CNC_STATUS_CHAIN_DISABLED 25
#define | CNC_STATUS_TIMEOUT 26
#define | CNC_STATUS_SFP_LOS 28
#define | CNC_STATUS_SFP_FAULT 29

## Macro Definition Documentation

## ◆ _REGISTERS_5215_H

#define _REGISTERS_5215_H

CAEN SpA - Front End Division Via Vetraia, 11 - 55049 - Viareggio ITALY +390594388398 - www.caen.it

Note
  TERMS OF USE: This program is free software; you can redistribute it and/or modify it under the terms of the GNU General Public License as published by the Free Software Foundation. This program is distributed in the hope that it will be useful, but WITHOUT ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. The user relies on the software, documentation and results solely at his own risk.

Definition at line 18 of file FERS_Registers_5215.h.

## ◆ VR_IO_STANDARD

#define VR_IO_STANDARD 0

Definition at line 24 of file FERS_Registers_5215.h.

## ◆ VR_IO_FA_DIR

#define VR_IO_FA_DIR 1

Definition at line 25 of file FERS_Registers_5215.h.

## ◆ VR_IO_FB_DIR

#define VR_IO_FB_DIR 2

Definition at line 26 of file FERS_Registers_5215.h.

## ◆ VR_IO_RA_DIR

#define VR_IO_RA_DIR 3

Definition at line 27 of file FERS_Registers_5215.h.

## ◆ VR_IO_RB_DIR

#define VR_IO_RB_DIR 4

Definition at line 28 of file FERS_Registers_5215.h.

## ◆ VR_IO_FA_FN

#define VR_IO_FA_FN 5

Definition at line 29 of file FERS_Registers_5215.h.

## ◆ VR_IO_FB_FN

#define VR_IO_FB_FN 6

Definition at line 30 of file FERS_Registers_5215.h.

## ◆ VR_IO_RA_FN

#define VR_IO_RA_FN 7

Definition at line 31 of file FERS_Registers_5215.h.

## ◆ VR_IO_RB_FN

#define VR_IO_RB_FN 8

Definition at line 32 of file FERS_Registers_5215.h.

## ◆ VR_IO_FOUT_FN

#define VR_IO_FOUT_FN 9

Definition at line 33 of file FERS_Registers_5215.h.

## ◆ VR_IO_VETO_FN

#define VR_IO_VETO_FN 10

Definition at line 34 of file FERS_Registers_5215.h.

## ◆ VR_IO_FIN_MASK

#define VR_IO_FIN_MASK 11

Definition at line 35 of file FERS_Registers_5215.h.

## ◆ VR_IO_FOUT_MASK

#define VR_IO_FOUT_MASK 12

Definition at line 36 of file FERS_Registers_5215.h.

## ◆ VR_IO_REG_VALUE

#define VR_IO_REG_VALUE 13

Definition at line 37 of file FERS_Registers_5215.h.

## ◆ VR_IO_TP_PERIOD

#define VR_IO_TP_PERIOD 14

Definition at line 38 of file FERS_Registers_5215.h.

## ◆ VR_IO_TP_WIDTH

#define VR_IO_TP_WIDTH 15

Definition at line 39 of file FERS_Registers_5215.h.

## ◆ VR_IO_CLK_SOURCE

#define VR_IO_CLK_SOURCE 16

Definition at line 40 of file FERS_Registers_5215.h.

## ◆ VR_IO_SYNC_OUT_A_FN

#define VR_IO_SYNC_OUT_A_FN 17

Definition at line 41 of file FERS_Registers_5215.h.

## ◆ VR_IO_SYNC_OUT_B_FN

#define VR_IO_SYNC_OUT_B_FN 18

Definition at line 42 of file FERS_Registers_5215.h.

## ◆ VR_IO_SYNC_OUT_C_FN

#define VR_IO_SYNC_OUT_C_FN 19

Definition at line 43 of file FERS_Registers_5215.h.

## ◆ VR_IO_MASTER_SALVE

#define VR_IO_MASTER_SALVE 20

Definition at line 44 of file FERS_Registers_5215.h.

## ◆ VR_IO_SYNC_PULSE_WIDTH

#define VR_IO_SYNC_PULSE_WIDTH 21

Definition at line 45 of file FERS_Registers_5215.h.

## ◆ VR_IO_SYNC_SEND

#define VR_IO_SYNC_SEND 22

Definition at line 46 of file FERS_Registers_5215.h.

## ◆ VR_SYNC_DELAY

#define VR_SYNC_DELAY 23

Definition at line 47 of file FERS_Registers_5215.h.

## ◆ VR_FIN_MAJORITY

#define VR_FIN_MAJORITY 24

Definition at line 48 of file FERS_Registers_5215.h.

## ◆ VR_IO_PPS_SOURCE

#define VR_IO_PPS_SOURCE 25

Definition at line 49 of file FERS_Registers_5215.h.

## ◆ VR_IO_PLL_STATUS

#define VR_IO_PLL_STATUS 26

Definition at line 50 of file FERS_Registers_5215.h.

## ◆ VR_IO_LED_TEST_1

#define VR_IO_LED_TEST_1 27

Definition at line 51 of file FERS_Registers_5215.h.

## ◆ VR_IO_LED_TEST_2

#define VR_IO_LED_TEST_2 28

Definition at line 52 of file FERS_Registers_5215.h.

## ◆ VR_DMA_FLAGS_INFO

#define VR_DMA_FLAGS_INFO 29

Definition at line 53 of file FERS_Registers_5215.h.

## ◆ VR_DMA_FLAGS_DATA

#define VR_DMA_FLAGS_DATA 30

Definition at line 54 of file FERS_Registers_5215.h.

## ◆ VR_ENABLED_LINKS

#define VR_ENABLED_LINKS 31

Definition at line 55 of file FERS_Registers_5215.h.

## ◆ VR_IO_DEBUG

#define VR_IO_DEBUG 32

Definition at line 56 of file FERS_Registers_5215.h.

## ◆ VR_IO_SYNCSOURCE_ZERO

#define VR_IO_SYNCSOURCE_ZERO 0

Definition at line 60 of file FERS_Registers_5215.h.

## ◆ VR_IO_SYNCSOURCE_SW_PULSE

#define VR_IO_SYNCSOURCE_SW_PULSE 1

Definition at line 61 of file FERS_Registers_5215.h.

## ◆ VR_IO_SYNCSOURCE_SW_REG

#define VR_IO_SYNCSOURCE_SW_REG 2

Definition at line 62 of file FERS_Registers_5215.h.

## ◆ VR_IO_SYNCSOURCE_FA

#define VR_IO_SYNCSOURCE_FA 3

Definition at line 63 of file FERS_Registers_5215.h.

## ◆ VR_IO_SYNCSOURCE_FB

#define VR_IO_SYNCSOURCE_FB 4

Definition at line 64 of file FERS_Registers_5215.h.

## ◆ VR_IO_SYNCSOURCE_RA

#define VR_IO_SYNCSOURCE_RA 5

Definition at line 65 of file FERS_Registers_5215.h.

## ◆ VR_IO_SYNCSOURCE_RB

#define VR_IO_SYNCSOURCE_RB 6

Definition at line 66 of file FERS_Registers_5215.h.

## ◆ VR_IO_SYNCSOURCE_GPS_PPS

#define VR_IO_SYNCSOURCE_GPS_PPS 7

Definition at line 67 of file FERS_Registers_5215.h.

## ◆ VR_IO_SYNCSOURCE_CLK_REF

#define VR_IO_SYNCSOURCE_CLK_REF 8

Definition at line 68 of file FERS_Registers_5215.h.

## ◆ VR_IO_BOARD_MODE_MASTER

#define VR_IO_BOARD_MODE_MASTER 0

Definition at line 70 of file FERS_Registers_5215.h.

## ◆ VR_IO_BOARD_MODE_SLAVE

#define VR_IO_BOARD_MODE_SLAVE 1

Definition at line 71 of file FERS_Registers_5215.h.

## ◆ VR_IO_STANDARD_IO_NIM

#define VR_IO_STANDARD_IO_NIM 0

Definition at line 73 of file FERS_Registers_5215.h.

## ◆ VR_IO_STANDARD_IO_TLL

#define VR_IO_STANDARD_IO_TLL 1

Definition at line 74 of file FERS_Registers_5215.h.

## ◆ VR_IO_DIRECTION_OUT

#define VR_IO_DIRECTION_OUT 0

Definition at line 76 of file FERS_Registers_5215.h.

## ◆ VR_IO_DIRECTION_IN_R50

#define VR_IO_DIRECTION_IN_R50 1

Definition at line 77 of file FERS_Registers_5215.h.

## ◆ VR_IO_DIRECTION_IN_HIZ

#define VR_IO_DIRECTION_IN_HIZ 2

Definition at line 78 of file FERS_Registers_5215.h.

## ◆ VR_IO_FUNCTION_REGISTER

#define VR_IO_FUNCTION_REGISTER 0

Definition at line 80 of file FERS_Registers_5215.h.

## ◆ VR_IO_FUNCTION_LOGIC_OR

#define VR_IO_FUNCTION_LOGIC_OR 1

Definition at line 81 of file FERS_Registers_5215.h.

## ◆ VR_IO_FUNCTION_LOGIC_AND

#define VR_IO_FUNCTION_LOGIC_AND 2

Definition at line 82 of file FERS_Registers_5215.h.

## ◆ VR_IO_FUNCTION_MAJORITY

#define VR_IO_FUNCTION_MAJORITY 3

Definition at line 83 of file FERS_Registers_5215.h.

## ◆ VR_IO_FUNCTION_TEST_PULSE

#define VR_IO_FUNCTION_TEST_PULSE 4

Definition at line 84 of file FERS_Registers_5215.h.

## ◆ VR_IO_FUNCTION_SYNC

#define VR_IO_FUNCTION_SYNC 5

Definition at line 85 of file FERS_Registers_5215.h.

## ◆ VR_IO_FUNCTION_FA_IN

#define VR_IO_FUNCTION_FA_IN 6

Definition at line 86 of file FERS_Registers_5215.h.

## ◆ VR_IO_FUNCTION_FB_IN

#define VR_IO_FUNCTION_FB_IN 7

Definition at line 87 of file FERS_Registers_5215.h.

## ◆ VR_IO_FUNCTION_RA_IN

#define VR_IO_FUNCTION_RA_IN 8

Definition at line 88 of file FERS_Registers_5215.h.

## ◆ VR_IO_FUNCTION_RB_IN

#define VR_IO_FUNCTION_RB_IN 9

Definition at line 89 of file FERS_Registers_5215.h.

## ◆ VR_IO_FUNCTION_ZERO

#define VR_IO_FUNCTION_ZERO 15

Definition at line 90 of file FERS_Registers_5215.h.

## ◆ VR_IO_CLKSOURCE_INTERNAL

#define VR_IO_CLKSOURCE_INTERNAL 0

Definition at line 92 of file FERS_Registers_5215.h.

## ◆ VR_IO_CLKSOURCE_LEMO

#define VR_IO_CLKSOURCE_LEMO 1

Definition at line 93 of file FERS_Registers_5215.h.

## ◆ VR_IO_CLKSOURCE_SYNC

#define VR_IO_CLKSOURCE_SYNC 2

Definition at line 94 of file FERS_Registers_5215.h.

## ◆ VR_IO_CLKSOURCE_RA

#define VR_IO_CLKSOURCE_RA 3

Definition at line 95 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_TX_SYNC_SHORT

#define VR_DPROBE_MON_TX_SYNC_SHORT 0x01

sending periodic synch (short)

Definition at line 98 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_TX_SYNC_ALIGN

#define VR_DPROBE_MON_TX_SYNC_ALIGN 0x02

link alignment in progress

Definition at line 99 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_TX_SYNC_LONG

#define VR_DPROBE_MON_TX_SYNC_LONG 0x03

sending periodic synch (long)

Definition at line 100 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_TX_TIMING_SEND

#define VR_DPROBE_MON_TX_TIMING_SEND 0x04

sending Timing *T0

Definition at line 101 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_TX_NORMAL_SEND

#define VR_DPROBE_MON_TX_NORMAL_SEND 0x05

FSM low level TX is in the state ready to transmit standard packets (reg/cmd)

Definition at line 102 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_TX_TLAST_SEND

#define VR_DPROBE_MON_TX_TLAST_SEND 0x06

FSM low level TX is transmetting last word.

Definition at line 103 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_TX_DATA_SEND

#define VR_DPROBE_MON_TX_DATA_SEND 0x07

FSM low level TX is transmetting a standard packets (reg/cmd)

Definition at line 104 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_TX_SYNC_PENDING

#define VR_DPROBE_MON_TX_SYNC_PENDING 0x08

Periodic synch is pending.

Definition at line 105 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_TX_FIFOFULL

#define VR_DPROBE_MON_TX_FIFOFULL 0x09

TX fifo full, commands and re access will be lost.

Definition at line 106 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_TX_TVALID

#define VR_DPROBE_MON_TX_TVALID 0x0A

tvalid fifo tx

Definition at line 107 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_TX_TREADY

#define VR_DPROBE_MON_TX_TREADY 0x0B

tready fifo tx

Definition at line 108 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_SC_BUSY

#define VR_DPROBE_SC_BUSY 0x10

register cmd interface busy

Definition at line 109 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_SC_DATA_WR

#define VR_DPROBE_SC_DATA_WR 0x11

data to write

Definition at line 110 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_SC_INT_RD

#define VR_DPROBE_SC_INT_RD 0x12

read operation request

Definition at line 111 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_SC_INT_WR

#define VR_DPROBE_SC_INT_WR 0x13

write operation request

Definition at line 112 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_SC_COMMIT

#define VR_DPROBE_SC_COMMIT 0x14

packet commit

Definition at line 113 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_SC_ACK

#define VR_DPROBE_SC_ACK 0x15

ack to commit request

Definition at line 114 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_SC_NACK

#define VR_DPROBE_SC_NACK 0x16

nack to commit request

Definition at line 115 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_STR_SOP

#define VR_DPROBE_STR_SOP 0x17

start incoming data packet

Definition at line 116 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_STR_EOP

#define VR_DPROBE_STR_EOP 0x18

end incoming data packet

Definition at line 117 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_STR_EOB

#define VR_DPROBE_STR_EOB 0x19

end of train

Definition at line 118 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_STR_DATA_VALID

#define VR_DPROBE_STR_DATA_VALID 0x20

data valid (read)

Definition at line 119 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_CMD_BUSY

#define VR_DPROBE_CMD_BUSY 0x21

command interface busy

Definition at line 120 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_CMD_COMMIT

#define VR_DPROBE_CMD_COMMIT 0x22

sending command from CPU

Definition at line 121 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_ENUMERATEBOARD

#define VR_DPROBE_ENUMERATEBOARD 0x23

request of enumeration

Definition at line 122 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_ENUMERATION_COMPLETED

#define VR_DPROBE_ENUMERATION_COMPLETED 0x24

enumeration completed

Definition at line 123 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_SEND_T0

#define VR_DPROBE_SEND_T0 0x25

send T0

Definition at line 124 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_G_REINIT_LINK

#define VR_DPROBE_G_REINIT_LINK 0x26

reinitialize link

Definition at line 125 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_READOUT_READY

#define VR_DPROBE_READOUT_READY 0x27

readout ready

Definition at line 126 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_AXSM_WRITEREG

#define VR_DPROBE_MON_AXSM_WRITEREG 0x30

FSM protocol is sending a reg read.

Definition at line 127 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_AXSM_READREG

#define VR_DPROBE_MON_AXSM_READREG 0x31

FSM protocol is sending a reg write.

Definition at line 128 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_AXSM_SENDCMD

#define VR_DPROBE_MON_AXSM_SENDCMD 0x32

FSM protocol is sending a command.

Definition at line 129 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_AXSM_SENDTOKEN

#define VR_DPROBE_MON_AXSM_SENDTOKEN 0x33

FSM protocol is sending a token (start of train)

Definition at line 130 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_AXSM_PENDING_TOKEN

#define VR_DPROBE_MON_AXSM_PENDING_TOKEN 0x34

a token is pending (= is circulating)

Definition at line 131 of file FERS_Registers_5215.h.

## ◆ VR_DPROBE_MON_AXSM_PENDING_REG

#define VR_DPROBE_MON_AXSM_PENDING_REG 0x35

pending send register

Definition at line 132 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_INVALID_CHAIN

#define CNC_STATUS_INVALID_CHAIN 1

Definition at line 135 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_INVALID_BOARD

#define CNC_STATUS_INVALID_BOARD 2

Definition at line 136 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_INVALID_FIRMWARE

#define CNC_STATUS_INVALID_FIRMWARE 3

Definition at line 137 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_CHAIN_NOT_INITIALIZED

#define CNC_STATUS_CHAIN_NOT_INITIALIZED 4

Definition at line 138 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_UNABLE_TO_MAP_MEMORY_TO_USER_SPACE

#define CNC_STATUS_UNABLE_TO_MAP_MEMORY_TO_USER_SPACE 5

Definition at line 139 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_UNABLE_TO_OPEN_DEV_MEM

#define CNC_STATUS_UNABLE_TO_OPEN_DEV_MEM 6

Definition at line 140 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_UNABLE_TO_ALLOCATE_USER_MEMORY

#define CNC_STATUS_UNABLE_TO_ALLOCATE_USER_MEMORY 7

Definition at line 141 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_UANBLE_TO_ALLOCATE_KERNEL_MEMORY

#define CNC_STATUS_UANBLE_TO_ALLOCATE_KERNEL_MEMORY 8

Definition at line 142 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_MEMORY_NOT_MAPPED

#define CNC_STATUS_MEMORY_NOT_MAPPED 9

Definition at line 143 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_ADDRESS_OUT_OF_MEMORY

#define CNC_STATUS_ADDRESS_OUT_OF_MEMORY 10

Definition at line 144 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_NO_MORE_SPACE

#define CNC_STATUS_NO_MORE_SPACE 11

Definition at line 145 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_EMPTY

#define CNC_STATUS_EMPTY 12

Definition at line 146 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_FULL

#define CNC_STATUS_FULL 13

Definition at line 147 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_INVALID_SETTINGS

#define CNC_STATUS_INVALID_SETTINGS 14

Definition at line 148 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_NO_MORE_SPACE_IN_THE_LIST

#define CNC_STATUS_NO_MORE_SPACE_IN_THE_LIST 15

Definition at line 149 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_LIST_ALMOST_FULL

#define CNC_STATUS_LIST_ALMOST_FULL 16

Definition at line 150 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_DMA_FAILED

#define CNC_STATUS_DMA_FAILED 17

Definition at line 151 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_CHAIN_DOWN

#define CNC_STATUS_CHAIN_DOWN 18

Definition at line 152 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_INVALID_IO_MODE

#define CNC_STATUS_INVALID_IO_MODE 19

Definition at line 153 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_FPGA_IO_ERROR

#define CNC_STATUS_FPGA_IO_ERROR 20

Definition at line 154 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_IIC_IO_ERROR

#define CNC_STATUS_IIC_IO_ERROR 21

Definition at line 155 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_INVALID_REGISTER

#define CNC_STATUS_INVALID_REGISTER 22

Definition at line 156 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_LINK_ERROR

#define CNC_STATUS_LINK_ERROR 23

Definition at line 157 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_UNABLE_TO_SET_LINK_PROP_DELAY

#define CNC_STATUS_UNABLE_TO_SET_LINK_PROP_DELAY 24

Definition at line 158 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_CHAIN_DISABLED

#define CNC_STATUS_CHAIN_DISABLED 25

Definition at line 159 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_TIMEOUT

#define CNC_STATUS_TIMEOUT 26

Definition at line 160 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_SFP_LOS

#define CNC_STATUS_SFP_LOS 28

Definition at line 161 of file FERS_Registers_5215.h.

## ◆ CNC_STATUS_SFP_FAULT

#define CNC_STATUS_SFP_FAULT 29

Definition at line 162 of file FERS_Registers_5215.h.