| CAEN FERS Library v1.1.4 SDK for FERS systems

Macros
Board constants
Macros

FERS board family constants. More...

Collaboration diagram for Board constants:

## Macros
#define | FERSLIB_MAX_NCNC 4
#define | FERSLIB_MAX_NBRD 128
#define | FERSLIB_MAX_NCH 128
#define | FERSLIB_MAX_NCH_5202 64
#define | FERSLIB_MAX_NCH_5203 128
#define | FERSLIB_MAX_NCH_5204 64
#define | PICOTDC_NCH 64
#define | FERSLIB_MAX_NTDL 8
#define | FERSLIB_MAX_NNODES 16

## Detailed Description

FERS board family constants.

## Macro Definition Documentation

## ◆ FERSLIB_MAX_NCNC

#define FERSLIB_MAX_NCNC 4

Max number of concentrators

Definition at line 125 of file FERSlib.h.

## ◆ FERSLIB_MAX_NBRD

#define FERSLIB_MAX_NBRD 128

Max number of connected boards

Definition at line 126 of file FERSlib.h.

## ◆ FERSLIB_MAX_NCH

#define FERSLIB_MAX_NCH 128

Max number of channels per board (for all boards)

Definition at line 127 of file FERSlib.h.

## ◆ FERSLIB_MAX_NCH_5202

#define FERSLIB_MAX_NCH_5202 64

Max number of channels per board

Definition at line 128 of file FERSlib.h.

## ◆ FERSLIB_MAX_NCH_5203

#define FERSLIB_MAX_NCH_5203 128

Max number of channels per board

Definition at line 129 of file FERSlib.h.

## ◆ FERSLIB_MAX_NCH_5204

#define FERSLIB_MAX_NCH_5204 64

Max number of channels per board

Definition at line 130 of file FERSlib.h.

## ◆ PICOTDC_NCH

#define PICOTDC_NCH 64

number of picoTDC channels

Definition at line 131 of file FERSlib.h.

## ◆ FERSLIB_MAX_NTDL

#define FERSLIB_MAX_NTDL 8

Max number of TDlinks (chains) in a concentrator

Definition at line 132 of file FERSlib.h.

## ◆ FERSLIB_MAX_NNODES

#define FERSLIB_MAX_NNODES 16

Max number of nodes in a TDL chain

Definition at line 133 of file FERSlib.h.