| CAEN FERS Library v1.1.4 SDK for FERS systems

Data Fields
FERS_CncInfo_t Struct Reference
FERS Library Structures » Board Info

Concentrator board information structure. More...

`#include <FERSlib.h>`

Collaboration diagram for FERS_CncInfo_t:

## Data Fields
uint32_t | pid
| Board PID (5 decimal digits) More...
char | PCBrevision [16]
| PCB revision. More...
char | ModelCode [16]
| Model code, e.g. WDT5215XAAAA. More...
char | ModelName [16]
| Model name, e.g. DT5215. More...
char | FPGA_FWrev [20]
| FPGA FW revision. More...
char | SW_rev [20]
| Software Revision (embedded ARM) More...
char | MACaddr_10GbE [20]
| MAC address of 10 GbE. More...
uint16_t | NumLink
| Number of links. More...
FERS_TDL_ChainInfo_t | ChainInfo [8]
| TDL Chain info. More...

## Detailed Description

Concentrator board information structure.

Definition at line 511 of file FERSlib.h.

## Field Documentation

## ◆ pid

uint32_t pid

Board PID (5 decimal digits)

Definition at line 512 of file FERSlib.h.

## ◆ PCBrevision

char PCBrevision[16]

PCB revision.

Definition at line 513 of file FERSlib.h.

## ◆ ModelCode

char ModelCode[16]

Model code, e.g. WDT5215XAAAA.

Definition at line 514 of file FERSlib.h.

## ◆ ModelName

char ModelName[16]

Model name, e.g. DT5215.

Definition at line 515 of file FERSlib.h.

## ◆ FPGA_FWrev

char FPGA_FWrev[20]

FPGA FW revision.

Definition at line 516 of file FERSlib.h.

## ◆ SW_rev

char SW_rev[20]

Software Revision (embedded ARM)

Definition at line 517 of file FERSlib.h.

## ◆ MACaddr_10GbE

char MACaddr_10GbE[20]

MAC address of 10 GbE.

Definition at line 518 of file FERSlib.h.

## ◆ NumLink

uint16_t NumLink

Number of links.

Definition at line 519 of file FERSlib.h.

## ◆ ChainInfo

FERS_TDL_ChainInfo_t ChainInfo[8]

TDL Chain info.

Definition at line 520 of file FERSlib.h.

The documentation for this struct was generated from the following file:

- FERSlib.h