| CAEN FERS Library v1.1.4 SDK for FERS systems

Data Fields
FERS_BoardInfo_t Struct Reference
FERS Library Structures » Board Info

FERS board information structure. More...

`#include <FERSlib.h>`

Collaboration diagram for FERS_BoardInfo_t:

## Data Fields
uint32_t | pid
| Board PID (5 decimal digits) More...
uint16_t | FERSCode
| FERS code, e.g. 5202. More...
uint8_t | PCBrevision
| PCB revision. More...
char | ModelCode [16]
| Model code, e.g. WA5202XAAAAA. More...
char | ModelName [16]
| Model name, e.g. A5202. More...
uint8_t | FormFactor
| Form factor (0=naked version (A52XX), 1=boxed version (DT52XX) More...
uint16_t | NumCh
| Number of channels. More...
uint32_t | FPGA_FWrev
| FPGA FW revision. More...
uint32_t | uC_FWrev
| Microcontroller (uC) FW revision. More...

## Detailed Description

FERS board information structure.

Definition at line 530 of file FERSlib.h.

## Field Documentation

## ◆ pid

uint32_t pid

Board PID (5 decimal digits)

Definition at line 531 of file FERSlib.h.

## ◆ FERSCode

uint16_t FERSCode

FERS code, e.g. 5202.

Definition at line 532 of file FERSlib.h.

## ◆ PCBrevision

uint8_t PCBrevision

PCB revision.

Definition at line 533 of file FERSlib.h.

## ◆ ModelCode

char ModelCode[16]

Model code, e.g. WA5202XAAAAA.

Definition at line 534 of file FERSlib.h.

## ◆ ModelName

char ModelName[16]

Model name, e.g. A5202.

Definition at line 535 of file FERSlib.h.

## ◆ FormFactor

uint8_t FormFactor

Form factor (0=naked version (A52XX), 1=boxed version (DT52XX)

Definition at line 536 of file FERSlib.h.

## ◆ NumCh

uint16_t NumCh

Number of channels.

Definition at line 537 of file FERSlib.h.

## ◆ FPGA_FWrev

uint32_t FPGA_FWrev

FPGA FW revision.

Definition at line 538 of file FERSlib.h.

## ◆ uC_FWrev

uint32_t uC_FWrev

Microcontroller (uC) FW revision.

Definition at line 539 of file FERSlib.h.

The documentation for this struct was generated from the following file:

- FERSlib.h